USB Media Card Reader

# User's Manual

General Note Package Contents System Requirement Product Applications Product Features | Hot Swapping Installation Guide for Windows 98/Win 98 SE/Windows 2000 for Windows ME / Windows XP For MAC OS 8.6 / 9.x For MAC OS X One Year Warranty Regulation Optional Accessories

General Note

This user's manual is written to assist users to install the product when it is first received and to attach the product to the USB port of host computer. The manufacturer reserves the right to make improvements to the product and to revise the document associated with it at anytime without notice.

BACK

Package Contents

The following items are included in the kit:

- USB Flash Memory Card Reader Unit
- Installation CD
- Quick Start sheet
- USB extension cable

BACK

System Requirements

To install the reader you need:

- One available USB port
- Windows 98, Windows 98SE, Windows Me, Windows 2000, Windows XP, Mac OS 8.6 / 9.x, OS X
- One available CD-ROM drive.
- 16MB RAM

BACK

Product Applications

USB Flash Memory Card Reader is designed to bridge between computer and Digital Cameras, Personal Digital assistants (PDA), Personal Organizers, Voice recorders, MP3 Players or other mobile electronic products using Flash Cards as standard or extended data storage media. USB Flash Memory Card Reader operates as a removable drive which allows you to download digital images and data instantly and easily to your computer.

BACK

Product Features

- Transfer Rate: 500-800KB/Sec. or higher depending on your system configuration.
- Power: DC + 5 Volts supplied by USB port.
- Easy to install and use; Simply plug and play.
- Remarkable high-speed digital image and data transfer to computer.
- Portable and convenient to carry around for mobile photography and computing.
- Draws power directly from USB port without need for auxiliary power sources (batteries or AC/DC adapter).
- Specifically designed for digital cameras and also ideally for using with Palmtop PCs, Handheld PCs, PDAs, Voice Recorders, MP3 Players and other mobile electronics using Flash Cards as standard or extended storage media.
- Hot swapping capacity for reinserting Flash card without restarting the computer system.

BACK

Optional Accessories

- CompactFlash Card.
- SmartMedia Card.
- MMC Card.
- SD Card.
- IBM MicroDrive.
- MemoryStick

The LCD will light on when the flash card is inserted into the slot.

BACK

Hot Swapping

USB Flash Memory Card Reader has the feature of hot swapping. Hot swapping allows you to remove and insert different Flash Cards without turning off host computer. The removal and insertion of different Flash Cards will be detected by computer automatically after device drivers have been installed to the computer.

BACK

Installation Guide

BACK

For Windows 98/ Windows 98 SE / Windows 2000

For Windows 2000 Before install the card reader, please install driver first, then plug in the card reader and reboot the computer.

1. Boot up computer .
2. Insert the software driver CD into your CD-ROM drive .
3. Wait for the pop-up menu to come out. If the pop-up menu doesn't come out automatically, please execute the autorun.exe file manually in the software driver CD from "My computer" icon then CD ROM drive icon.
4. Click "Install Software Driver" Lable on the pop-up menu.
5. Follow the instructions to complete the Setup program and restart the computer .
6. Connect Image Card Reader to computer, make sure all the cables are well connected.
7. The USB Flash Memory Card Reader will be recognized as four Removable Disk icons in "MY COMPUTER".

BACK

Windows ME, Windows XP

1. Boot up computer .
2. Connect the USB Flash Memory Card Reader to computer.
3. The USB Flash Memory Card Reader will be recognized as four Removable Disk icons in "MY COMPUTER".

Remove Card Reader (For Windows ME / Windows 2000 /Windows XP )

1. Double click the "Removable Device" icon to show the "Unplug or Eject Hardware" window.

1. Choose the "USB Disk" (the one you'd like to remove) and press "Stop" button to pop up the "Stop a Hardware device" window.
2. Press "OK" button to pop up the "Remove Hardware" window.
3. Press "OK" button to eject the USB Disk.
4. Repeat step 1 ~ step 4 to remove other USB Disks.

BACK

For Macintosh OS 8.6 / 9.x:

1. Insert the enclosed installation CD into the CD-ROM drive.
2. The installer icon of "Reader" will appear.
3. Double click on the installer of "Reader" to install the drivers.
4. Follow on-screen instructions to complete installation.
5. Restart the system to activate the Reader.
6. Plug the USB Flash Memory Card Reader in the USB port.
7. Slide a Flash Memory Card in the Reader.
8. The Reader will be recognized as four "UNTITLED" drive icons on the Screen.

For Macintosh OS X :

No driver is required. The reader will be detected automatically

BACK

!!!!!!!!!!!!!Important notice for Mac users:!!!!!!!!!!!!!!!!!!!!!!!!!!

1. To be safe, always drag and drop the "Untitled" drive icon into trash can before you remove the Flash Card from the reader or unplug the reader from USB port.

2. If the system hangs due to improper operation, unplug the reader and remove Flash Card then restart the system. When the system is back on, plug in the reader first then insert Flash Memory Card in the reader.
3. Formatting the Flash Memory Card in the Mac might cause compatibility issues. Please use Digital Camera to format the Flash Memory Card.

!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!

Installation is complete.

Congratulations, you have successfully installed the USB Flash Memory Card Reader. Now, you are ready to read and write your Flash Memory cards.

BACK

One Year Warranty Regulation

This product is to be warranted to be free from defects in material and workmanship under the following terms:

- The effective period of this warranty is ONE year for parts and labor from the date of customer purchase.
- The maker is responsible only to repair or replace any defective hardware component part of such products.
- The buyer is obliged to pay shipping cost of sending defective products to the maker.

The warranty will not apply when

- Any product, on which the serial number has been defaced, modified or removed.
- Malfunction damage, deterioration resulting from accident, misuse, neglect, fire, water, or other act of nature, unauthorized product modification or failure to follow instructions supplied with the product.
- Damage or other loss in any shipment.

BACK